****

**POS13（i5 4G／128G）**

|  |  |
| --- | --- |
| **Configuration（Model：POS13）** | |
| Cabinet size | 460mm(W)\*300mm(L)\*420mm(H) |
| Main Board | Industrial POS motherboard |
| CPU | i5 2.70 GHZ |
| Memory | DDR 4G |
| Hard Disk | 128G SSD |
| Color | Black （Same as photo） |
| Power supply | 12V/5A 250W/220V/110V ATX Power supply |
| Interface | USB\*6 / Lan \* 1 / HDMI \*1 / VGA \*1 / Audio in and out \* 1 |
| Monitor | 15.6-inch LED screen panel |
| Touch Screen | Capacitive Screen |
| Customer display | 15'' TFT LCD Resolution |
| POS keyboard(optional) | NCTS-KB2 keyboard  (Optional: NCTS-KB95 pos keyboard with magcard reader track2+3,or programmable keyboard with magcard reader track2+3) |
| Barcode scanner(optional) | CCD barcode scanners or Laser barcode scanners/2D scanners |
| Label Printer(optional) | Industrial or Not-industrial label printer |
| POS Software（optional） | Retail or restaurant POS software |
| Operation System(optional) | Win XP, Win 7, 8, 10 |
| Carton box size | 470mm(W)\*310mm(L)\*430mm(H) |
| N.W. | 6KG |
| G.W | 7KG |